Hot Work Checklist
Date: _______________________   Time: _____________________
Name of Person(s) Performing Work:
______________________________________________________________________________

Specific Location of Work: ______________________    Duration of Permit: ________________

	Yes
	No
		

	
	
	Cutting or welding permitted in an area that has been made fire safe.

	
	
	All movable fire hazards in the vicinity have been taken to a safe place.

	
	
	Guards used to contain the heat, sparks, and slag if fire hazards cannot be removed.

	
	
	Floor or wall openings or cracks, open doorways and windows protected or closed.

	
	
	Fire extinguisher available for instant use.

	
	
	Fire watch in areas where other than a minor fire might develop such as around combustible material.

	
	
	Floors swept clean of combustible material for a radius of 10.5 m (35 ft).

	
	
	Combustible floors have been kept wet, covered with damp sand or protected by fire resistant shields.

	
	
	Welding/cutting done only in areas authorized by management. No welding/cutting in sprinkled building when sprinkler system is impaired or in presence of explosive atmosphere, or in area of storage of readily ignitable material.

	
	
	Dusts and conveyor systems that might carry sparks to distant combustibles protected or shutdown.

	
	
	Cutter/welder is trained in safe operation of equipment and the safe use of the process.

	
	
	Any on-site contractors advised about flammable material or hazardous conditions of which they may not be aware.

	
	
	Welding or cutting containers:
Container thoroughly cleaned and ventilated;
Any pipe lines or connections to containers disconnected or blanked.

	
	
	PPE used as needed, e.g., eye protection, helmet, protective clothing, respirator, gloves.

	
	
	Warning sign posted to warn other workers of hot metal.

	
	
	Appropriate ventilation provided.

	
	
	When working in confined spaces a permit must be issued for this as well.




	_______________________________________
	Authorized Signature
